# Samsung Specific repair steps

## S8

### Screen

1. Heat adhesive
2. Suction back
3. Patiently cut adhesive
4. Reheat if needed
5. Carefully disconnect fingerprint sensor
6. Take back off
7. Unscrew NFC antenna and charging coil assembly plate
8. Unscrew Loudspeaker
9. Disconnect Battery
10. Disconnect Screen
11. Heat adhesive
12. Suction front
13. Patiently cut adhesive
14. Reheat if needed
15. Connect new Screen
16. Put everything back together

### Battery

1. Heat adhesive
2. Suction back
3. Patiently cut adhesive
4. Reheat if needed
5. Carefully disconnect fingerprint sensor
6. Take back off
7. Unscrew NFC antenna and charging coil assembly plate
8. Disconnect battery
9. Heat adhesive under battery
10. Replace battery
11. Put everything back together

## S9

### Screen

1. Heat adhesive
2. Suction back
3. Patiently cut adhesive
4. Reheat if needed
5. Carefully disconnect fingerprint sensor
6. Take back off
7. Unscrew NFC antenna and charging coil assembly plate
8. Unscrew Loudspeaker
9. Disconnect Battery
10. Disconnect Screen
11. Heat adhesive
12. Suction front
13. Patiently cut adhesive
14. Reheat if needed
15. Remove Battery
16. Remove motherboard and other components
17. Connect new Screen
18. Put everything back together

## S10

### Screen

1. Heat adhesive
2. Suction back
3. Patiently cut adhesive
4. Reheat if needed
5. Take back off
6. Unscrew NFC antenna and charging coil assembly plate
7. Unscrew Loudspeaker
8. Disconnect Battery
9. Disconnect Screen
10. Heat adhesive
11. Suction front
12. Patiently cut adhesive
13. Reheat if needed
14. Remove Battery
15. Remove motherboard and other components
16. Connect new Screen
17. Put everything back together